@incollection{MARTIN19771,
title = {Heat and Mass Transfer between Impinging Gas Jets and Solid Surfaces},
editor = {James P. Hartnett and Thomas F. Irvine},
series = {Advances in Heat Transfer}, booktitle = {Advances in Heat Transfer},
publisher = {Elsevier},
volume = {13},
pages = {1-60},
year = {1977},
issn = {0065-2717},
doi = {https://doi.org/10.1016/S0065-2717(08)70221-1},
url = {https://www.sciencedirect.com/science/article/pii/S0065271708702211},
author = {Holger Martin},
abstract = {Publisher Summary
Heating or cooling of large surface area products is often carried out in devices consisting of arrays of round or slot nozzles, through which air impinges vertically upon the product surface. This chapter presents a comprehensive survey emphasizing the engineering applications and empirical equations, presented for the prediction of heat and mass transfer coefficients within a large and technologically important range of variables. The local variations of the transfer coefficients are based on the experimental data for single round nozzles (SRN), arrays of round nozzles (ARN), single slot nozzles (SSN), and arrays of slot nozzles (ASN). The variation of local transfer coefficients is graphically represented. It also explores how to apply these equations in heat exchanger and dryer design as well as in optimization. The flow field of impinging flow is diagrammatically represented. External variables influencing heat and mass transfer in impinging flow depends on mass flow rate, kind and state of the gas and on the shape, size, and position of the nozzles relative to each other and to the solid surface. The design of high-performance arrays of nozzles is also discussed.}
}
@article{Kaczmarek2007,
author = { Mariusz   Kaczmarek  and  Antoni   Nowakowski  and  Marek   Suchowirski  and  Janusz   Siebert  and  Wojciech   Stojek },
title = {Active dynamic thermography in cardiosurgery},
journal = {Quantitative InfraRed Thermography Journal},
volume = {4},
number = {1},
pages = {107-123},
year  = {2007},
publisher = {Taylor & Francis},
doi = {10.3166/qirt.4.107-123},

URL = { 
        https://doi.org/10.3166/qirt.4.107-123
    
},
eprint = { 
        https://doi.org/10.3166/qirt.4.107-123
    
}
}
@inproceedings{inproceedings,
author = {St-Laurent, Louis and Prévost, Donald and Maldague, X.},
year = {2010},
month = {01},
pages = {},
title = {Fast and accurate calibration-based thermal / colour sensors registration},
booktitle = {Proceedings of the 10th International Conference on Quantitative InfraRed Thermography},
doi = {10.21611/qirt.2010.126}
}
@article{RENKIELSKA2006867,
title = {Burn depths evaluation based on active dynamic IR thermal imaging—A preliminary study},
journal = {Burns},
volume = {32},
number = {7},
pages = {867-875},
year = {2006},
issn = {0305-4179},
doi = {https://doi.org/10.1016/j.burns.2006.01.024},
url = {https://www.sciencedirect.com/science/article/pii/S0305417906000374},
author = {Alicja Renkielska and Antoni Nowakowski and Mariusz Kaczmarek and Jacek Ruminski},
keywords = {Active dynamic IR thermal imaging, Burn depth, Diagnosis},
abstract = {Proper diagnostic assessment of burn wound depth is of the highest importance in selecting the mode of burn wound treatment. Several diagnostic methods – clinical and histopathological evaluation, as well as methods employing IR imaging – static thermography and active dynamic thermography (ADT) – are compared on the basis of in vivo experiments conducted on three domestic pigs (23 burn wounds). ADT is presented here as a new, reliable and quantitative method of assessing burn wound depth on the basis of discrimination of the thermal properties of burnt tissue. In the case of ADT registration of thermal images was performed following thermal pulse excitation. A series of captured infrared images was used as the basis for calculating the thermal time constant τ for each pixel. The parameter values were compared with histopathological and clinical assessments of burn depth. The mean value of τ was found for burns, which heal within 3 weeks (τ=12.08±1.94s) and for burns, which did not heal during this period (τ=9.07±0.68s), p<0.05. The accuracy, sensitivity and specificity of all the methods tested were compared, the best results coming from ADT. The ADT method is fast, non-invasive and relatively inexpensive, although it still requires further animal experimentation as well as clinical study to confirm the results.}
}